


# Manual for D/A Conversion



1. Function: Custom channel type by user
2. Support model : H265 ADVR
3. Usage



Such as the below picture shown, you could change the analog channel type A8 to digital channel type: Click the icon  in A8,



you can switch the digital type(D1) to analog type, click  in D1,



1. Note:

* A means Analog(Local mode),D means Digital (IP mode)
* Most models’ local mode can support D/A conversion function, please refer to the specific model.